# Panasonic DMC-FZ100 remote and timelaps

Board and software to control ypur DMC-FZ100 with a Raspberry PI, threw the remote port.

## Remote connector connectics
![remote resistors](docs/remote_resistor.gif)

## Requierement 

Configure SPI port with ```raspi-config```

## Build 
```gcc src/timelaps_raspberry.c -o timelaps_raspberry```



